
30T Timing Gear - 16T Pinion
	Runs at 1rev/60sec
	16T Pinion meshes with 60T Gear2

60T Gear2-15T Pinion2
	Runs at 1rev/(3.75*60)sec = 1rev/225sec
	15T Pinion meshes with 60T Gear3

60T Gear3-15T Pinion3
	Runs at 1rev/(4*225)sec = 1rev/900sec
	15T Pinion meshes with 60T Gear4
	
60T Gear4-15T Pinion4
	Runs at 1rev/(4*900)sec = 1rev/3600sec = 1rev/60min = 1rev/hr
	15T Pinion meshes with the 60T Weight Gear5

10T Pinion7
	Attached to Gear4-Pinion4 Shaft, runs at 1rev/60min
	10T Pinion7 meshes with 30T Gear6
	
30T Gear6-8T Pinion6
	Runs at 1rev/(3*60min) = 1rev/180min
	8T Pinion6 meshes with 32T Gear7 and Hour Hand
	
32T Gear 7
	Runs at 1rev/(4*180)min = 1rev/720min = 1rev/12hr
		
60T Weight Gear 5
	Meshes with 15T Pinion 4
	Runs at 1rev/(4*60)min = 1rev/240min = 1rev/4hr

Minute Hand is attached to Gear4 Shaft
Hour Hand is attatched to Gear 7

	
Weight Drum Dia = 35mm	Circumference = 110mm
Rotation speed = 1rev/4hr
With 1m (1000mm) of cord, runtime = 36.36hr


